Trim Boards and Soffit Panels (per building)

Trim boards inside of building:

22 – 1x4x12 – No paint for ceiling

6 – 1x4x12 – Body colour for baseboard

2 – 1x4x8 – Body colour for baseboard

5 – 1x4x8 – Body colour for door trim

16 – 1x4x8 – Body colour for window trim

Trim boards outside of building:

4 – 1x4x12 – Trim colour for belly bands

8 – 1x4x8 – Trim colour for window trim

8 – 1x4x8 – Trim colour for corners

Totals:

32 – 1x4x12

39 – 1x4x8

Plywood:

8 sheets per building painted for soffit panels